anti electronic warfare solution

when the frequency is being hacked by the enemy and the signal starts to be lost, the frequency is automatically changed to another one,

coordinated between the drone and the control system.

the encryption will make sure that both system work in the same frequency

the best encryption is like the SE-135/235

the frequeny is changed thousend times per seconds, following the encryption system.

Python :

learn how to deploy a rasberry pi with Debian and Python installed in it

know how to use crotab

use ymal file as configuration files with inputs

ensure the raspberry pi is secured

connect to the RPi through Wi-fi

access it and modify the python program running on it

Python API

binance

Manga

connect to different links, one per series

each time we read, we mark the last chapter

the python scripts connects to the links and checks if a new chapter is available. if yes, the panel highlights the new chapter and the link to read it with the default browser.

in the log, the last chapter number is saved. if new chapters appear, the script displays a list with links to the new chapter. the user has only to click on the links to read them.

in front of each link, we have a button for the user, he clicks on it when the chapter is red.