Ballistics

compute the Reynold number at each moment to define the regime of the fluid : laminar, intermediary or turbulant.

Python : fluid\_mode : 'laminar', 'intermediary, 'turbulant'

for each regime, define the correct formula for the fluid drag, ....

in the intermediary regime, a mix of laminar and turbulant